EWFC baseline revision history

## Release 1.8B 09-06-16

AUTHOR: Cervati M.

NOTES:

CHANGES:

* Add Defrosting 8 programmable interval time
* Add 2 alternative defrosting mode (1 mode- first defrost after a compressor stop and the others after a timeout, 2 mode- first defrost at a settable time and the others after a timeout)
* Add external digital input defrosting command on DI8
* In a recovery state from a power fail event, the cycle is repeated if it was present before power fail (storing cycle in

BUG FIXES:

* In frame defrosting display the Index of list parameters has RW property, instead RO.

KNOWN ISSUES:

* HACCP managing is not present yet. In a power fail case it need to check the time and the temperature in the power on state.

## Release 1.8A 22-06-15

AUTHOR: Marcassa F - Tremonti T.

NOTES:

* Starting release

CHANGES:

* Quick chiller application

BUG FIXES:

KNOWN ISSUES: